# 2D Barcode FMX Components

## Installation

1. Before installing the components package, please close all RAD Studio (Delphi and C++ Builder) IDEs.

   Note, for each IDE, if it's a clean installation, please run it at least once before installing the components package, then closes it and continues installation.

2. Run the installation file barcodefmx2d_tri.exe, and then click on the "Next" button in the installation dialog box.
3. Read the End-User License Agreement. You must accept the terms of this agreement before continuing with the installation. And then click on the "Next" button.
4. Specify a target folder (it will be created if does not exist), the components package will be installed into it. And then click on the "Next" button.
5. All supported RAD Studio (Delphi and C++ Builder) IDEs will be listed automatically. Please select the IDEs you want to install to them. And then click on the "Next" button.
6. Specify a shortcuts folder in "Start Menu" for the components package. And then click on the "Next" button. Later, you can open the manual or remove the components package in the shortcuts folder.
7. Click on the "Install" button to complete the components package installation.
8. Click on the "Finish" button to close the installation dialog box.
9. You can start your IDE to use the components package now.

## Note:

- If multi-user accounts want to use the components package, please install it into the same folder in each user session.
- All of 32-bit Windows, 64-bit Windows, 32-bit Mac OSX, 64-bit Mac OSX (X86 & ARM), 32-bit iOS, 64-bit iOS, 32-bit Android, 64-bit Android components are included (depend on the version of your RAD Studio).

Copyright © 2001-2026 Han-soft Corporation. All rights reserved.